GSIC - Global Service Information Center

# REAR SHOCK ABSORBER (for 4WD) > REMOVAL

## for Preparation Click here

HINT:

1. Use the same procedures for the RH side and LH side.

1. The procedures listed below are for the LH side.

1. A bolt without a torque specification is shown in the standard bolt chart.

1. REMOVE REAR WHEEL

2. REMOVE REAR SHOCK ABSORBER ASSEMBLY

1. Support the rear axle housing.

   1. Jack up and support the vehicle's frame on stands.

   2. Lower the axle housing until the leaf spring tension is free, and maintain this position.

1. Remove the 2 bolts and 2 washers.

1. Disconnect the absorber (with the 4 bushes) from the U bolt seat and frame.

1. Remove the 4 bushes from the absorber.

1. Remove the 2 washers.