GSIC - Global Service Information Center

# FRONT BRAKE (for 2WD) > REMOVAL

## for Preparation Click here

HINT:

1. Use the same procedures for the LH side and RH side.
2. The procedures listed below are for the LH side.

1. REMOVE FRONT WHEEL

2. DRAIN BRAKE FLUID

NOTICE:

  Wash off brake fluid immediately if it comes in contact with any painted surface.

3. REMOVE FRONT FLEXIBLE HOSE

1. Remove the union bolt and gasket.

1. Disconnect the flexible hose from the brake cylinder.

4. REMOVE DISC BRAKE CYLINDER ASSEMBLY LH

1. Remove the 2 bolts and cylinder.