GSIC - Global Service Information Center

# PARKING BRAKE CABLE (for 2WD) > REMOVAL

## for Preparation Click here

1. DISCONNECT CABLE FROM NEGATIVE BATTERY TERMINAL

CAUTION:

  Wait at least 90 seconds after disconnecting the cable from the negative (-) battery terminal to prevent airbag and seat belt pretensioner activation.

2. REMOVE REAR WHEEL

3. REMOVE REAR BRAKE DRUM SUB-ASSEMBLY

4. REMOVE SHIFT LEVER KNOB SUB-ASSEMBLY

5. REMOVE PARKING BRAKE HOLE COVER SUB-ASSEMBLY

1. Detach the 4 claws and remove the hole cover.

6. REMOVE UPPER CONSOLE PANEL SUB-ASSEMBLY

NOTICE:

  Be careful not to damage the instrument panel lower and console box with the claws of the console panel upper.

1. Detach the 12 claws and remove the console panel.

7. REMOVE CONSOLE BOX ASSEMBLY

1. Remove the 4 screws <F> and 2 bolts <E>.

1. Using a clip remover, remove the 2 clips and console box.

8. REMOVE NO. 1 PARKING BRAKE CABLE ASSEMBLY

1. Disconnect the cable from the parking brake lever (Click here).

1. Remove the 2 bolts and No. 1 heat insulator.

1. Remove the No. 1 clip and pin labeled A.

1. Disconnect the cable from the No. 3 cable.

1. Disconnect the cable from the equalizer labeled B.

1. Remove the bolt holding the cable labeled C.

1. Remove the cable from the cable support bracket labeled D.

9. REMOVE NO. 2 PARKING BRAKE CABLE ASSEMBLY

1. Disconnect the cable from the parking brake shoe lever RH and backing plate RH.

   1. Disconnect the cable from the lever (Click here).

   2. Remove the 2 bolts and disconnect the cable from the backing plate.

1. Disconnect the cable from the equalizer labeled A.

1. Remove the 4 bolts labeled B and cable.

10. REMOVE NO. 3 PARKING BRAKE CABLE ASSEMBLY

1. Disconnect the cable from the parking brake shoe lever LH and backing plate LH.

   1. Disconnect the cable from the lever (Click here).

   2. Remove the 2 bolts and disconnect the cable from the backing plate.

1. Remove the No. 3 clip labeled A.

1. Remove the 4 bolts labeled B, nut labeled C and cable.