GSIC - Global Service Information Center

# BRAKE PEDAL > REASSEMBLY

## for Preparation Click here

1. INSTALL BRAKE PEDAL PAD

1. Install the pad to the pedal.

2. INSTALL STOP LIGHT SWITCH ASSEMBLY

1. Install the adjuster to the support.

1. Insert the switch into the adjuster until it slightly touches the pedal.

   NOTICE:
     Do not depress the pedal.

1. Turn the switch a quarter turn clockwise.

   Torque:
     1.5 N*m{ 15 kgf*cm , 13 in.*lbf } or less

   NOTICE:
     Do not depress the pedal.

1. Connect the switch connector to the switch.

1. Check the switch clearance.

   Stop light switch clearance:
     1.5 to 2.5 mm (0.059 to 0.098 in.)

3. INSTALL BRAKE PEDAL SUB-ASSEMBLY

1. Apply lithium soap base glycol grease to 2 new bushes and the shaft.

1. Install the pedal and 2 bushes to the support with the shaft and nut.

   Torque:
     37 N*m{ 377 kgf*cm , 27 ft.*lbf }