GSIC - Global Service Information Center

# FRONT SUSPENSION LOWER ARM (for 4WD) > DISASSEMBLY

## for Preparation Click here

1. REMOVE FRONT NO. 1 LOWER ARM BUSH

1. Using a hammer and chisel, strike and bend the entire flange of the bush as shown in the illustration.

1. Using SST and a press, press out the bush.

   SST
     09632-36010
     09950-00020
     09950-60010 (09951-00520)

2. REMOVE FRONT NO. 2 LOWER ARM BUSH

1. Using a hammer and chisel, strike and bend the entire flange of the bush as shown in the illustration.

1. Using SST and a press, press out the bush.

   SST
     09632-36010
     09950-00020
     09950-60010 (09951-00400)