GSIC - Global Service Information Center

# CLUTCH MASTER CYLINDER > REMOVAL

## for Preparation Click here

1. DRAIN CLUTCH FLUID

2. REMOVE INSTRUMENT CLUSTER FINISH PANEL

1. Remove the clip.

1. Detach the 2 claws and remove the panel.

3. REMOVE COMBINATION METER ASSEMBLY

NOTICE:

  There are 2 types of combination meters. One type has a 40 pin connector and 16 pin connector. The other type only has a 40 pin connector.

1. Remove the 3 screws <B>.

1. Disconnect all connectors and remove the combination meter.

4. DISCONNECT CLUTCH RESERVOIR HOSE

1. Using pliers, grip the claws of the clip, slide the clip and disconnect the clutch reservoir hose.

   HINT:
     Use a container to catch the fluid.

5. DISCONNECT CLUTCH MASTER CYLINDER TO FLEXIBLE TUBE

1. Using SST, disconnect the flexible tube.

   SST
     09023-00101

   HINT:
     Use a container to catch the fluid.

6. REMOVE CLUTCH MASTER CYLINDER ASSEMBLY

1. Remove the clutch pedal.
   For LHD (Click here)
   For RHD (Click here)

1. Remove the clutch master cylinder and gasket.