GSIC - Global Service Information Center

# POWER WINDOW REGULATOR MOTOR > ON-VEHICLE INSPECTION

## for Preparation Click here

1. INSPECT POWER WINDOW REGULATOR MOTOR ASSEMBLY (FRONT LH)

1. Apply battery voltage to connector terminals 1 and 2.

   NOTICE:
     Do not apply battery voltage to any terminals except terminals 1 and 2.

1. Check that the motor gear rotates smoothly as follows.

   OK:

     Measurement Condition | Specified Condition
     Battery positive (+) → 1 Battery negative (-) → 2 | Motor gear rotates counterclockwise
     Battery positive (+) → 2 Battery negative (-) → 1 | Motor gear rotates clockwise

   1. If the result is not as specified, replace the regulator motor assembly.

2. INSPECT POWER WINDOW REGULATOR MOTOR ASSEMBLY (FRONT RH)

1. Apply battery voltage to connector terminals 1 and 2.

   NOTICE:
     Do not apply battery voltage to any terminals except terminals 1 and 2.

1. Check that the motor gear rotates smoothly as follows.

   OK:

     Measurement Condition | Specified Condition
     Battery positive (+) → 1 Battery negative (-) → 2 | Motor gear rotates clockwise
     Battery positive (+) → 2 Battery negative (-) → 1 | Motor gear rotates counterclockwise

   1. If the result is not as specified, replace the regulator motor assembly.

3. INSPECT POWER WINDOW REGULATOR MOTOR ASSEMBLY (REAR LH)

1. Apply battery voltage to connector terminals 1 and 2.

1. Check that the motor gear rotates smoothly as follows.

   OK:

     Measurement Condition | Specified Condition
     Battery positive (+) → 1 Battery negative (-) → 2 | Motor gear rotates clockwise
     Battery positive (+) → 2 Battery negative (-) → 1 | Motor gear rotates counterclockwise

   1. If the result is not as specified, replace the regulator motor assembly.

4. INSPECT POWER WINDOW REGULATOR MOTOR ASSEMBLY (REAR RH)

1. Apply battery voltage to connector terminals 1 and 2.

1. Check that the motor gear rotates smoothly as follows.

   OK:

     Measurement Condition | Specified Condition
     Battery positive (+) → 1 Battery negative (-) → 2 | Motor gear rotates counterclockwise
     Battery positive (+) → 2 Battery negative (-) → 1 | Motor gear rotates clockwise

   1. If the result is not as specified, replace the regulator motor assembly.