GSIC - Global Service Information Center

# PARK / NEUTRAL POSITION SWITCH > INSPECTION

## for Preparation Click here

1. INSPECT PARK/NEUTRAL POSITION SWITCH

1. Measure the resistance of the PNP switch when the shift lever is moved to each position.

   Standard resistance:

     Tester Connection | Shift Lever Position | Specified Condition
     4 (B) - 5 (L) | P or N | Below 1 Ω
     4 (B) - 5 (L) | Not on P or N | 10 kΩ or higher
     1 (RL) - 2 (RB) | R | Below 1 Ω
     1 (RL) - 2 (RB) | Not on R | 10 kΩ or higher
     2 (RB) - 7 (DL) | D | Below 1 Ω
     2 (RB) - 7 (DL) | Not on D | 10 kΩ or higher
     2 (RB) - 3 (2L) | 2 | Below 1 Ω
     2 (RB) - 3 (2L) | Not on 2 | 10 kΩ or higher
     2 (RB) - 8 (LL) | L | Below 1 Ω
     2 (RB) - 8 (LL) | Not on L | 10 kΩ or higher