GSIC - Global Service Information Center

# REAR COMBINATION LIGHT ASSEMBLY > INSTALLATION

## for Preparation Click here

HINT:

1. Use the same procedures for the RH and LH side.
2. The procedures listed below are for the LH side.

1. INSTALL REAR COMBINATION LIGHT BULB

1. Turn the 3 bulbs in the direction indicated by the arrows to install them.

2. INSTALL REAR COMBINATION LIGHT ASSEMBLY

1. Connect the connector.

1. Attach the rear combination light with the 2 clips.

1. Install the 2 screws.

3. CONNECT CABLE TO NEGATIVE BATTERY TERMINAL

4. PERFORM INITIALIZATION

1. Perform initialization (Click here ).

   NOTICE:
     Certain systems need to be initialized after disconnecting and reconnecting the cable from the negative (-) battery terminal.