GSIC - Global Service Information Center

# REAR BUMPER (for Step Type) > DISASSEMBLY

## for Preparation Click here

1. REMOVE REAR BUMPER PLATE

1. Using a screwdriver, detach the 13 claws and remove the bumper plate from the bumper bar.

   HINT:
     Tape the screwdriver tip before use.

2. REMOVE REAR BUMPER PLATE LH

1. Using a screwdriver, detach the 7 claws and remove the bumper plate from the bumper bar.

   HINT:
     Tape the screwdriver tip before use.

3. REMOVE REAR BUMPER PLATE RH

HINT:

  Use the same procedures described for the LH side.