GSIC - Global Service Information Center

### RADIATOR > REMOVAL

1. DISCONNECT CABLE FROM NEGATIVE BATTERY TERMINAL

2. REMOVE RADIATOR GRILLE

3. REMOVE RADIATOR SIDE DEFLECTOR LH

4. REMOVE RADIATOR SIDE DEFLECTOR RH

5. REMOVE NO. 1 ENGINE UNDER COVER

6. DRAIN ENGINE COOLANT

7. REMOVE RADIATOR HOSE INLET

8. REMOVE RADIATOR HOSE OUTLET

9. REMOVE AIR PUMP INLET (for Unleaded Gasoline Specification Vehicle)

10. REMOVE FAN SHROUD

11. DISCONNECT NO. 1 OIL COOLER TUBE INLET (for Automatic Transmission)

12. DISCONNECT NO. 1 OIL COOLER TUBE OUTLET (for Automatic Transmission)

13. REMOVE RADIATOR ASSEMBLY