GSIC - Global Service Information Center

# EXTENSION HOUSING REAR OIL SEAL > REMOVAL

## for Preparation Click here

1. REMOVE PROPELLER SHAFT WITH CENTER BEARING ASSEMBLY

1. Remove the propeller shaft with center bearing assembly (Click here).

2. DRAIN AUTOMATIC TRANSMISSION FLUID

1. Remove the drain plug, gasket and drain ATF.

1. Install a new gasket and the drain plug.

   Torque:
     28 N*m{ 285 kgf*cm , 21 ft.*lbf }

3. REMOVE AUTOMATIC TRANSMISSION EXTENSION HOUSING OIL SEAL

1. Using SST, remove the oil seal.

   SST
     09308-00010