GSIC - Global Service Information Center

# CRANKSHAFT POSITION SENSOR > INSPECTION

## for Preparation Click here

1. INSPECT CRANKSHAFT POSITION SENSOR

1. Measure the resistance between terminals 1 and 2.

   Standard resistance:

     Temperature | Specified Condition
     Cold | 1,630 to 2,740 Ω
     Hot | 2,065 to 3,225 Ω

   NOTICE:
     In the table above, the terms "cold" and "hot" refer to the temperature of the coils. "Cold" means approximately -10 to 50°C (14 to 122°F). "Hot" means approximately 50 to 100°C (122 to 212°F).
   If the resistance is not as specified, replace the sensor.