GSIC - Global Service Information Center

# FUEL TEMPERATURE SENSOR > INSPECTION

## for Preparation Click here

1. INSPECT FUEL TEMPERATURE SENSOR

1. Measure the resistance between the terminals.

   Standard resistance:

     Condition | Specified Condition
     Approx. 20°C (68°F) | 2.21 to 2.69 kΩ
     Approx. 80°C (176°F) | 0.287 to 0.349 kΩ

   NOTICE:
     When checking the fuel temperature sensor in the water, keep the terminals dry. After the check, wipe the sensor dry.
   If the result is not as specified, replace the sensor.