GSIC - Global Service Information Center

# IGNITION KEY CYLINDER LIGHT > INSPECTION

## for Preparation Click here

1. INSPECT TRANSPONDER KEY AMPLIFIER

1. Inspect operation of the ignition key cylinder lamp.

   1. Connect the battery's positive (+) lead to terminal 2 and negative (-) lead to terminal 6. Then check that the LED illuminates.

      OK:
        LED illuminates.
      If the result is not as specified, replace the transponder key amplifier.