GSIC - Global Service Information Center

# OIL PUMP > REPLACEMENT

## for Preparation Click here

1. REMOVE ENGINE FRONT OIL SEAL

1. Using a screwdriver and hammer, tap out the oil seal.

2. REMOVE SUPPLY PUMP OIL SEAL

1. Using a screwdriver and hammer, tap out the oil seal.

3. INSTALL SUPPLY PUMP OIL SEAL

1. Using SST and a hammer, tap in a new oil seal until its surface is flush with the timing gear cover edge.

   SST
     09223-15020
     09502-12010
     09950-70010 (09951-07100)

1. Apply MP grease to the oil seal lip.

4. INSTALL ENGINE FRONT OIL SEAL

1. Using SST and a hammer, tap in a new oil seal until its surface is flush with the timing gear cover edge.

   SST
     09214-76011

1. Apply MP grease to the oil seal lip.