GSIC - Global Service Information Center

### STEERING KNUCKLE (for 2WD) > REMOVAL

1. REMOVE FRONT WHEEL

2. REMOVE FRONT SPEED SENSOR

3. REMOVE FRONT DISC BRAKE CALIPER ASSEMBLY LH

4. REMOVE FRONT DISC

5. DISCONNECT TIE ROD END SUB-ASSEMBLY LH

6. DISCONNECT FRONT SUSPENSION LOWER ARM ASSEMBLY WITH ATTACHMENT LH

7. DISCONNECT FRONT SUSPENSION UPPER ARM ASSEMBLY LH

8. REMOVE FRONT AXLE HUB ASSEMBLY

9. REMOVE KNUCKLE GREASE RETAINER CAP

10. REMOVE FRONT AXLE HUB NUT AND ABS SPEED SENSOR ROTOR OR SPACER

11. REMOVE FRONT AXLE HUB SUB-ASSEMBLY LH

12. REMOVE FRONT AXLE HUB OIL SEAL

13. REMOVE FRONT AXLE HUB INNER BEARING