GSIC - Global Service Information Center

### DTC P2716 Pressure Control Solenoid "D" Electrical (Shift Solenoid Valve SLT)

## for Preparation Click here

## DESCRIPTION

(Click here).

DTC No. | DTC Detection Condition | Trouble Area

P2716

Open or short is detected in shift solenoid valve SLT circuit for 1 second or more while driving (1 trip detection logic)

1. Open or short in shift solenoid valve SLT circuit
2. Shift solenoid valve SLT
3. ECM

## MONITOR DESCRIPTION

When an open or short in the linear solenoid valve SLT circuit is detected, the ECM interprets this as a fault. The ECM will illuminate the MIL and store the DTC.

## WIRING DIAGRAM

## INSPECTION PROCEDURE

1.INSPECT TRANSMISSION WIRE (SHIFT SOLENOID VALVE SLT)

1. Disconnect the E1 wire connector.

1. Measure the resistance of the wire connector.

   Standard resistance:

     Tester Connection | Condition | Specified Condition
     14 (SLT+) - 6 (SLT-) | 20°C (68°F) | 5.0 to 5.6 Ω
     14 (SLT+) - Body ground | 20°C (68°F) | 10 kΩ or higher
     6 (SLT-) - Body ground | 20°C (68°F) | 10 kΩ or higher

| NG |

Go to step 3

OK |

2.CHECK WIRE HARNESS (TRANSMISSION WIRE - ECM)

1. Disconnect the E16 ECM connector.

1. Measure the resistance of the wire harness side connector.

   Standard resistance:

     Tester Connection | Condition | Specified Condition
     E16-13 (SLT+) - E16-12 (SLT-) | 20°C (68°F) | 5.0 to 5.6 Ω
     E16-13 (SLT+) - Body ground | 20°C (68°F) | 10 kΩ or higher
     E16-12 (SLT-) - Body ground | 20°C (68°F) | 10 kΩ or higher

| NG |

REPAIR OR REPLACE HARNESS AND CONNECTOR

OK |

REPLACE ECM

3.INSPECT SHIFT SOLENOID VALVE SLT

1. Remove the shift solenoid valve SLT.

1. Measure the resistance of the solenoid valve.

   Standard resistance:
     5.0 to 5.6 Ωat 20°C (68°F)

1. Connect the battery's positive (+) lead to the terminal of the solenoid connector, and the negative (-) lead to the solenoid body.

   OK:
     Solenoid makes operating noise.

   HINT:

     Reference: Inspect using an oscilloscope.
     Check the waveform of the ECM connector.

   Standard voltage:
     Refer to illustration.

     Item | Content
     Tester Connection | E16-13 (SLT+) - E16-12 (SLT-)
     Tool Setting | 5 V/DIV., 1 msec./DIV.
     Condition | Engine idle speed

| NG |

REPLACE SHIFT SOLENOID VALVE SLT

OK |

REPAIR OR REPLACE TRANSMISSION WIRE