GSIC - Global Service Information Center

# DRIVE BELT > ON-VEHICLE INSPECTION

## for Preparation Click here

1. INSPECT DRIVE BELT

1. Visually check the drive belt for excessive wear frayed cords, etc.
   If any defect is found, replace the drive belt.

   HINT:
     Cracks on the rib side of a drive belt are considered acceptable.
   If the drive belt has chunks missing from the ribs, it should be replaced.

2. INSPECT V-RIBBED BELT TENSIONER

1. Check that nothing gets caught in the tensioner by turning it clockwise and counterclockwise.
   If a malfunction exists, replace the tensioner.