GSIC - Global Service Information Center

# FUEL COOLER > INSTALLATION

## for Preparation Click here

1. INSTALL FUEL COOLER (for 2WD)

1. Install the cooler (with radio earth bracket) with the 3 nuts.

   Torque:
     7.5 N*m{ 76.5 kgf*cm , 66 in.*lbf }

1. Connect the 2 fuel hoses.

2. INSTALL FUEL COOLER (for 4WD)

1. Install the cooler with the 3 nuts.

   Torque:
     7.5 N*m{ 76.5 kgf*cm , 66 in.*lbf }

1. Connect the 2 fuel hoses.

3. ADD FUEL

4. TIGHTEN FUEL TANK CAP ASSEMBLY

5. BLEED AIR FROM FUEL SYSTEM

1. Using the hand pump, bleed air from the fuel system until pumping becomes difficult.

6. CHECK FOR FUEL LEAKS