GSIC - Global Service Information Center

# LOWER INSTRUMENT PANEL > INSTALLATION

## for Preparation Click here

HINT:

  A bolt without a torque specification is shown in the standard bolt chart (Click here).

1. INSTALL INSTRUMENT PANEL SUB-ASSEMBLY LOWER

1. Install the hood lock control cable lever and fuel lid control cable lever.

1. Connect all connectors, and attach all clamps to install the panel.

1. Install the panel with the 3 screws <F>, 2 bolts <A> and nut <G>.

2. INSTALL COWL SIDE TRIM BOARD LH

1. Install the cowl side trim board LH (Click here or Click here or Click here).

3. INSTALL COWL SIDE TRIM BOARD RH

1. Install the cowl side trim board RH (Click here or Click here or Click here).

4. INSTALL FRONT DOOR SCUFF PLATE LH

1. Install the front door scuff plate LH (Click here or Click here or Click here).

5. INSTALL FRONT DOOR SCUFF PLATE RH

1. Install the front door scuff plate RH (Click here or Click here or Click here).

6. INSTALL SWITCH BASE

1. Connect all connectors.

1. Attach the 8 claws to install the switch base.

7. INSTALL NO. 1 INSTRUMENT PANEL BOX

1. Connect all connectors.

1. Attach all clamps to install the panel box.

1. Install the panel box with the 6 screws <B> and 2 clips.

8. INSTALL CONSOLE BOX ASSEMBLY

1. Install the console box with the 2 clips, 4 screws <F> and 2 bolts <E>.

9. INSTALL CONSOLE PANEL SUB-ASSEMBLY UPPER

NOTICE:

  Be careful not to damage the instrument panel lower and console box with the claws of the console panel upper.

1. Attach the 12 claws to install the console panel.

10. INSTALL PARKING BRAKE HOLE COVER SUB-ASSEMBLY

1. Attach the 4 claws to install the hole cover.

11. INSTALL SHIFT LEVER KNOB SUB-ASSEMBLY

1. w/ M/T:
   Twist the knob in the direction indicated by the arrow to install it.

1. w/ 4WD:
   Twist the transfer shift lever knob in the direction indicated by the arrow to install it.

12. INSTALL INSTRUMENT PANEL FINISH PANEL SUB-ASSEMBLY LOWER

1. Attach the 2 claws and 3 clips to install the panel.

13. INSTALL HEADLIGHT DIMMER SWITCH ASSEMBLY

1. Install the headlight dimmer switch with the claw as shown in the illustration.

1. Install the headlight dimmer switch with the clamp.

1. Connect the connector.

14. INSTALL WINDSHIELD WIPER SWITCH ASSEMBLY

1. Attach the claw to install the wiper switch.

1. Connect the connectors.

   NOTICE:
     Do not push the claw with excessive force as damage may occur.

15. INSTALL INSTRUMENT PANEL SUB-ASSEMBLY UPPER

1. Install the instrument panel sub-assembly upper (Click here).

16. CONNECT CABLE TO NEGATIVE BATTERY TERMINAL

17. PERFORM INITIALIZATION

1. Perform initialization (Click here).

   NOTICE:
     Certain systems need to be initialized after disconnecting and reconnecting the cable from the negative (-) battery terminal.

18. CHECK SRS WARNING LIGHT

1. Check the SRS warning light (Click here).