GSIC - Global Service Information Center

# DIESEL THROTTLE BODY > INSTALLATION

## for Preparation Click here

1. INSTALL DIESEL THROTTLE BODY ASSEMBLY

1. Install a new gasket and the throttle body with the 2 bolts and 2 nuts.

   Torque:
     20 N*m{ 204 kgf*cm , 15 ft.*lbf }

1. Connect the 2 connectors.

2. INSTALL NO. 2 AIR CLEANER PIPE SUB-ASSEMBLY

1. Connect the pipe (with the 2 air hoses) and install the bolt.

   Torque:
     20 N*m{ 204 kgf*cm , 15 ft.*lbf }

1. Tighten the 2 clamps.

1. Connect the vacuum hose to the gas filter.

1. Connect the manifold absolute pressure sensor connector.

3. CONNECT CABLE TO NEGATIVE BATTERY TERMINAL

4. PERFORM INITIALIZATION

1. Perform initialization (Click here).

   NOTICE:
     Certain systems need to be initialized after disconnecting and reconnecting the cable from the negative (-) battery terminal.