GSIC - Global Service Information Center

### TURBOCHARGER > REMOVAL

1. DISCONNECT CABLE FROM NEGATIVE BATTERY TERMINAL

2. REMOVE NO. 1 ENGINE UNDER COVER

3. REMOVE FRONT WHEEL RH

4. REMOVE FRONT EXHAUST PIPE ASSEMBLY

5. REMOVE FRONT FENDER APRON SEAL UPPER

6. REMOVE FRONT FENDER SEAL

7. REMOVE VENTILATION HOSE HEAT INSULATOR

8. REMOVE AIR CLEANER ASSEMBLY

9. REMOVE NO. 2 AIR CLEANER PIPE SUB-ASSEMBLY

10. REMOVE TURBINE OUTLET ELBOW

11. REMOVE TURBOCHARGER SUB-ASSEMBLY