GSIC - Global Service Information Center

# GENERATOR > INSTALLATION

## for Preparation Click here

1. INSTALL GENERATOR ASSEMBLY

1. Install the generator and adjusting bar with the 2 bolts.

   Torque:
     62 N*m{ 630 kgf*cm , 46 ft.*lbf } for bolt A
     25 N*m{ 254 kgf*cm , 19 ft.*lbf } for bolt B

1. Install the generator wire with the nut.

   Torque:
     6.0 N*m{ 61 kgf*cm , 53 in.*lbf }

1. Connect the generator connector.

2. INSTALL FAN AND GENERATOR V BELT

1. Use the pulley set bolt of the tensioner to rotate the tensioner pulley clockwise, and then install the V belt.

   NOTICE:
     Make sure that the V belt is set properly at each pulley.

1. Make sure that the indicator mark of the tensioner is within range A, as shown in the illustration.

3. INSTALL AIR CLEANER ASSEMBLY

1. Connect the air cleaner hose.

1. Install the air cleaner with the 2 bolts.

   Torque:
     14 N*m{ 143 kgf*cm , 10 ft.*lbf }

1. Tighten the clamp.

1. Install the clamp and connect the IAT connector.

1. Connect the ventilation hose.

1. Slide the clamp to the connection of the hose.

4. CONNECT CABLE TO NEGATIVE BATTERY TERMINAL

5. PERFORM INITIALIZATION

1. Perform initialization (Click here).

   NOTICE:
     Certain systems need to be initialized after disconnecting and reconnecting the cable from the negative (-) battery terminal.