GSIC - Global Service Information Center

### DTC P0606 ECM / PCM Processor

### DTC P0607/89 Control Module Performance

### DTC P1611/17 Run Pulse Malfunction

## for Preparation Click here

## DESCRIPTION

DTC No. | DTC Detection Condition | Trouble Area
P0606 P0607/89 P1611/17 | ECM internal error (1 trip detection logic) | ECM

## INSPECTION PROCEDURE

HINT:

  Read freeze frame data using the intelligent tester. Freeze frame data records the engine condition when a malfunction is detected. When troubleshooting, freeze frame data can help determine if the vehicle was moving or stationary, if the engine was warmed up or not, and other data from the time the malfunction occurred.

NOTICE:

  If the ECM is replaced, the new ECM needs initialization (Click here).

1.CHECK OTHER DTC OUTPUT (IN ADDITION TO DTC P0606 OR P0607/89 OR P1611/17)

Result:

  Display (DTC output) | Proceed to
  P0606 or P0607/89 or P1611/17 | A
  P0606 or P0607/89 or P1611/17 and other DTCs | B

| B |

GO TO RELEVANT DTC CHART

A |

REPLACE ECM