GSIC - Global Service Information Center

# REAR COMBINATION LIGHT ASSEMBLY > REMOVAL

## for Preparation Click here

HINT:

1. Use the same procedures for the RH and LH side.
2. The procedures listed below are for the LH side.

1. DISCONNECT CABLE FROM NEGATIVE BATTERY TERMINAL

CAUTION:

  Wait at least 90 seconds after disconnecting the cable from the negative (-) battery terminal to prevent airbag and seat belt pretensioner activation.

2. REMOVE REAR COMBINATION LIGHT ASSEMBLY

1. Remove the 2 screws.

1. Detach the 2 clips and remove the lamp.

1. Disconnect the connector.

3. REMOVE REAR COMBINATION LIGHT BULB

1. Turn the 3 bulbs in the direction indicated by the arrows and pull to remove them.