GSIC - Global Service Information Center

# REAR SHOCK ABSORBER (for 4WD) > INSTALLATION

## for Preparation Click here

1. INSTALL REAR SHOCK ABSORBER ASSEMBLY

1. Install the 2 washers to the axle housing.

1. Install 4 new bushes to the absorber.

1. Install the absorber (with the 4 bushes) to the U bolt seat and frame.

1. Install the 2 washers.

1. Temporarily tighten the 2 bolts.

2. INSTALL REAR WHEEL

1. Install the wheel.

   Torque:
     105 N*m{ 1,070 kgf*cm , 77 ft.*lbf }

3. STABILIZE SUSPENSION

1. Lower the vehicle.

1. Press down on the vehicle several times to stabilize the suspension.

4. TIGHTEN REAR SHOCK ABSORBER BOLT

1. Tighten the 2 bolts.

   Torque:
     105 N*m{ 1,070 kgf*cm , 77 ft.*lbf }