GSIC - Global Service Information Center

# IGNITION SWITCH > INSPECTION

## for Preparation Click here

1. INSPECT IGNITION OR STARTER SWITCH ASSEMBLY

1. Measure the resistance of the switch.

   Standard resistance:

     Tester Connection | Switch Condition | Specified Condition
     - | LOCK | 10 kΩ or higher
     2 (ACC) - 4 (AM1) | ACC | Below 1 Ω
     1 (IG1) - 4 (AM1) 2 (ACC) - 4 (AM1) 5 (AM2) - 6 (IG2) | ON | Below 1 Ω
     1 (IG1) - 4 (AM1) 2 (ACC) - 4 (AM1) 5 (AM2) - 6 (IG2) 5 (AM2) - 7 (ST2) | START | Below 1 Ω

   If the result is not as specified, replace the ignition switch assembly.