GSIC - Global Service Information Center

# FRONT AIRBAG SENSOR > REMOVAL

## for Preparation Click here

CAUTION:

  Be sure to read the precautionary notices concerning the SRS airbag system before servicing (Click here).

1. DISCONNECT CABLE FROM NEGATIVE BATTERY TERMINAL

CAUTION:

  Wait at least 90 seconds after disconnecting the cable from the negative (-) battery terminal to prevent airbag and seat belt pretensioner activation.

2. REMOVE RADIATOR GRILLE

1. Using a clip remover, remove the 2 clips.

1. Remove the 2 screws.

1. Pull the radiator grille in the direction indicated by the arrow in the illustration to detach the 5 claws and remove the radiator grille.

3. REMOVE BATTERY (LH SENSOR)

1. Disconnect the cable from the positive (+) battery terminal.

1. Remove the 2 bolts and battery stay.

1. Remove the battery.

4. REMOVE AIR CLEANER ASSEMBLY (RH SENSOR)

5. REMOVE FRONT AIRBAG SENSOR LH

1. Remove the nut and sensor.

1. Disconnect the sensor connector.

6. REMOVE FRONT AIRBAG SENSOR RH

1. Remove the nut and sensor.

1. Disconnect the sensor connector.