GSIC - Global Service Information Center

# IGNITION KEY CYLINDER LIGHT > INSTALLATION

## for Preparation Click here

1. INSTALL TRANSPONDER KEY AMPLIFIER

1. Using a screwdriver, widen the claw hanging onto the upper bracket by approximately 1.0 mm (0.039 in.).

1. Pull out the transponder key amplifier with the claw open.

2. INSTALL STEERING COLUMN COVER UPPER

1. Install the cover lower with the 3 screws.

   Torque:
     2.0 N*m{ 20 kgf*cm , 18 in.*lbf }

3. INSTALL STEERING COLUMN COVER LOWER

1. Install the cover lower with the 3 screws.

   Torque:
     2.0 N*m{ 20 kgf*cm , 18 in.*lbf }

4. INSTALL STEERING WHEEL ASSEMBLY

1. Align the matchmarks on the steering wheel and main shaft.

1. Install the steering set nut.

   Torque:
     50 N*m{ 510 kgf*cm , 37 ft.*lbf }

5. PLACE FRONT WHEELS FACING STRAIGHT AHEAD

6. INSPECT STEERING WHEEL CENTER POINT

7. INSTALL STEERING PAD ASSEMBLY

1. Straighten the front wheels.

1. Using a T30 "torx" socket, loosen the 2 screws until the groove along each screw circumference catches on the screw case.

1. Pull out the steering pad from the steering wheel and support the steering pad with one hand as shown in the illustration.

   NOTICE:
     When removing the steering pad, do not pull the airbag wire harness.

1. Using a screwdriver, disconnect the airbag connector.

   CAUTION:
     When handling the airbag connector, do not damage the airbag wire harness.

1. Disconnect the horn connector and remove the steering pad.

8. CONNECT CABLE TO NEGATIVE BATTERY TERMINAL

9. INSPECT STEERING PAD ASSEMBLY

1. Check for cuts, cracks or discoloration on the steering pad outer surface and in the grooved portion.

1. Check that the horn sounds.

10. PERFORM INITIALIZATION

1. Perform initialization (Click here ).

   NOTICE:
     Certain systems need to be initialized after disconnecting and reconnecting the cable from the negative (-) battery terminal.

11. CHECK SRS WARNING LIGHT

1. Check the SRS warning light (Click here).