GSIC - Global Service Information Center

# FRONT SHOCK ABSORBER WITH COIL SPRING (for 4WD) > INSPECTION

## for Preparation Click here

1. INSPECT FRONT SHOCK ABSORBER ASSEMBLY

1. Compress and extend the shock absorber rod 4 times or more. Check there is no abnormal resistance or unusual sound during the operation.

   1. If there is any abnormality, replace the shock absorber assembly with a new one.

      NOTICE:
        When disposing of the shock absorber (Click here).