GSIC - Global Service Information Center

# BLOWER UNIT > INSTALLATION

## for Preparation Click here

1. INSTALL BLOWER ASSEMBLY

1. Connect the blower unit to the A/C radiator.

1. Install the blower assembly with the 3 bolts.

1. Install the nut.

   Torque:
     9.8 N*m{ 100 kgf*cm , 7 ft.*lbf }

2. INSTALL INSTRUMENT PANEL REINFORCEMENT

1. Install the instrument panel reinforcement with the 7 bolts.

   Torque:
     20 N*m{ 204 kgf*cm , 15 ft.*lbf }

1. Install the 3 bolts.

   Torque:
     9.8 N*m{ 100 kgf*cm , 7 ft.*lbf }

1. Connect the connectors.

1. Attach the 12 clamps.

1. Install the grommet to the vehicle body.

1. Connect the ground wires to the instrument panel reinforcement with the 2 bolts.

1. Connect the connector and wire harness.

1. w/o PTC heater:
   Attach the 2 clamps.

1. w/ PTC heater:
   Attach the 3 clamps.

1. Connect the connector and wire harness.

1. Attach the 2 clamps.

3. INSTALL NO. 4 AIR DUCT

1. Attach the 2 claws to install the duct.

4. INSTALL ECM

For 1TR-FE (Click here)
For 2TR-FE (Click here)
For 1GR-FE (Click here)
For 1KD-FTV (Click here)
For 2KD-FTV (Click here)

5. INSTALL NO. 1 INSTRUMENT PANEL BRACE SUB-ASSEMBLY

1. Connect the connectors to install the instrument panel junction block.

1. Attach the 2 clamps to install the brace.

1. Install the brace with the 3 nuts and 2 bolts.

6. INSTALL STEERING COLUMN ASSEMBLY

1. Install the steering column with the 3 bolts.

   Torque:
     21 N*m{ 214 kgf*cm , 15 ft.*lbf }

7. INSTALL NO. 3 HEATER TO REGISTER DUCT

1. Attach the 4 claws to install the duct.

8. INSTALL NO. 1 HEATER TO REGISTER DUCT

1. Attach the 3 claws to install the duct.

9. INSTALL NO. 2 HEATER TO REGISTER DUCT

1. Install the clip and duct.

10. INSTALL INSTRUMENT PANEL SUB-ASSEMBLY LOWER

1. Install the instrument panel sub-assembly lower (Click here).

11. INSTALL INSTRUMENT PANEL SUB-ASSEMBLY UPPER

1. Install the instrument panel sub-assembly upper (Click here).

12. CONNECT CABLE TO NEGATIVE BATTERY TERMINAL

13. PERFORM INITIALIZATION

1. Perform initialization (Click here).

   NOTICE:
     Certain systems need to be initialized after disconnecting and reconnecting the cable from the negative (-) battery terminal.

14. CHECK SRS WARNING LIGHT

1. Check the SRS warning light (Click here).