GSIC - Global Service Information Center

# REAR DOOR > ON-VEHICLE INSPECTION

## for Preparation Click here

1. INSPECT REAR DOOR PANEL SUB-ASSEMBLY LH

1. Check that the clearance measurements of areas A to I are within the standard range.

   Standard:

     Area | Measurement | Area | Measurement
     A | 5.0 +- 1.5 mm (0.197 +- 0.059 in.) | E | 4.6 +- 1.5 mm (0.181 +- 0.059 in.)
     B | 5.1 +- 1.5 mm (0.201 +- 0.059 in.) | F | 9.1 +- 1.5 mm (0.358 +- 0.059 in.)
     C | 2.3 +- 1.5 mm (0.091 +- 0.059 in.) | G | 4.3 +- 1.5 mm (0.169 +- 0.059 in.)
     D | 0.7 +- 1.5 mm (0.028 +- 0.059 in.) | H | 4.4 +- 1.5 mm (0.173 +- 0.059 in.)
     |  | - | -