GSIC - Global Service Information Center

# TRANSMISSION WIRE > INSTALLATION

## for Preparation Click here

1. INSTALL TRANSMISSION WIRE

1. Install the transmission wire with the bolt.

   Torque:
     5.4 N*m{ 55 kgf*cm , 48 in.*lbf }

1. Connect the transmission wire connector.

2. CONNECT TRANSMISSION WIRE

1. Connect the 7 connectors to the solenoid valves.

1. Install the clamp with the 2 bolts.

   Torque:
     10 N*m{ 100 kgf*cm , 7 ft.*lbf } for bolt A
     11 N*m{ 110 kgf*cm , 8 ft.*lbf } for bolt B

   Bolt length:
     36 mm (1.42 in.) for bolt A
     12 mm (0.47 in.) for bolt B

1. Connect the ATF temperature sensor.

3. INSTALL VALVE BODY OIL STRAINER ASSEMBLY

1. Install a new O-ring and oil strainer with the 4 bolts.

   Torque:
     10 N*m{ 100 kgf*cm , 7 ft.*lbf }

4. INSTALL AUTOMATIC TRANSMISSION OIL PAN SUB-ASSEMBLY

HINT:

  Remove the gasket and be careful not to spill oil on the contacting surfaces of the transmission case and oil pan.

1. Install the oil pan with the 20 bolts.

   Torque:
     4.4 N*m{ 45 kgf*cm , 39 in.*lbf }

5. CONNECT CABLE TO NEGATIVE BATTERY TERMINAL

6. PERFORM INITIALIZATION

1. Perform initialization (Click here).

   NOTICE:
     Certain systems need to be initialized after disconnecting and reconnecting the cable from the negative (-) battery terminal.

7. ADD AUTOMATIC TRANSMISSION FLUID

1. Add automatic transmission fluid (Click here).

8. INSPECT AUTOMATIC TRANSMISSION FLUID

1. Inspect the automatic transmission fluid (Click here).