GSIC - Global Service Information Center

### CAMSHAFT (for Bank 2) > REMOVAL

1. DISCONNECT BATTERY NEGATIVE TERMINAL

2. DRAIN ENGINE COOLANT

3. REMOVE V-BANK COVER

4. DISCONNECT NO. 2 VENTILATION HOSE

5. REMOVE AIR CLEANER

6. REMOVE INTAKE AIR SURGE TANK

7. REMOVE IGNITION COIL

8. REMOVE CYLINDER HEAD COVER RH

9. REMOVE CYLINDER HEAD COVER LH

10. SET NO. 1 CYLINDER TO TDC/COMPRESSION

11. REMOVE NO. 1 CHAIN TENSIONER

12. REMOVE NO. 4 CAMSHAFT

13. REMOVE NO. 3 CHAIN TENSIONER

14. REMOVE NO. 3 CAMSHAFT