GSIC - Global Service Information Center

# GLOW PLUG > INSTALLATION

## for Preparation Click here

1. INSTALL GLOW PLUG ASSEMBLY

1. Using a 12 mm deep socket wrench, install the 4 glow plugs.

   Torque:
     13 N*m{ 133 kgf*cm , 10 ft.*lbf }

2. INSTALL NO. 1 GLOW PLUG CONNECTOR

1. Install the glow plug connector by uniformly tightening the 4 nuts.

   Torque:
     2.2 N*m{ 22 kgf*cm , 19 in.*lbf }

1. Install the 4 screw grommets.

1. Install the wire harness with the nut.

   Torque:
     2.0 N*m{ 20 kgf*cm , 18 in.*lbf }

3. INSTALL INTAKE AIR CONNECTOR

1. Install a new gasket and the air connector with the 2 nuts and bolt.

   Torque:
     20 N*m{ 204 kgf*cm , 15 ft.*lbf }

4. INSTALL THROTTLE BODY BRACKET

1. Install the bracket with the 3 bolts.

   Torque:
     20 N*m{ 204 kgf*cm , 15 ft.*lbf }

5. INSTALL DIESEL THROTTLE BODY ASSEMBLY

1. Install a new gasket and the throttle body with the 2 bolts and 2 nuts.

   Torque:
     20 N*m{ 204 kgf*cm , 15 ft.*lbf }

1. Connect the 2 connectors.

6. INSTALL VACUUM SWITCHING VALVE BRACKET

1. Install the bracket with the 2 bolts.

   Torque:
     20 N*m{ 204 kgf*cm , 15 ft.*lbf }

7. INSTALL NO. 2 AIR CLEANER PIPE SUB-ASSEMBLY

1. Connect the pipe (with the 2 air hoses) and install the bolt.

   Torque:
     20 N*m{ 204 kgf*cm , 15 ft.*lbf }

1. Tighten the 2 clamps.

1. Connect the vacuum hose to the gas filter.

1. Connect the manifold absolute pressure sensor connector.

8. CONNECT CABLE TO NEGATIVE BATTERY TERMINAL

9. PERFORM INITIALIZATION

1. Perform initialization (Click here).

   NOTICE:
     Certain systems need to be initialized after disconnecting and reconnecting the cable from the negative (-) battery terminal.