GSIC - Global Service Information Center

# HIGH MOUNTED STOP LIGHT ASSEMBLY > REMOVAL

## for Preparation Click here

1. DISCONNECT CABLE FROM NEGATIVE BATTERY TERMINAL

CAUTION:

  Wait at least 90 seconds after disconnecting the cable from the negative (-) battery terminal to prevent airbag and seat belt pretensioner activation.

2. REMOVE TAIL GATE SERVICE HOLE COVER

1. Using a T30 "torx" socket, remove the 10 screws and cover.

3. REMOVE CENTER STOP LIGHT ASSEMBLY

1. Disconnect the connector.

1. Detach the 4 claws and remove the light.