GSIC - Global Service Information Center

# AIR CONDITIONING AMPLIFIER > INSTALLATION

## for Preparation Click here

1. INSTALL AIR CONDITIONING AMPLIFIER ASSEMBLY

1. Install the A/C amplifier with the screw.

1. Connect the connector.

1. Attach the clamp.

2. CONNECT CABLE TO NEGATIVE BATTERY TERMINAL

3. PERFORM INITIALIZATION

1. Perform initialization (Click here).

   NOTICE:
     Certain systems need to be initialized after disconnecting and reconnecting the cable from the negative (-) battery terminal.