GSIC - Global Service Information Center

# 2TR-FE EXHAUST > TORQUE SPECIFICATIONS

Part Tightened | N*m | kgf*cm | ft.*lbf
Front exhaust pipe x Air fuel ratio sensor : for use with SST | 40 | 408 | 30
Front exhaust pipe x Heated oxygen sensor : for use with SST | 40 | 408 | 30
Front exhaust pipe x Air fuel ratio sensor | 44 | 449 | 32
Front exhaust pipe x Heated oxygen sensor | 44 | 449 | 32
Front exhaust pipe x Turbine outlet elbow | 43 | 438 | 32
Front exhaust pipe x Center exhaust pipe | 48 | 489 | 35
Center exhaust pipe x Tailpipe | 48 | 489 | 35