GSIC - Global Service Information Center

# VALVE BODY ASSEMBLY > REASSEMBLY

## for Preparation Click here

1. INSTALL SHIFT SOLENOID VALVE

1. Install the shift solenoid valve S2 with the bolt.

   Torque:
     10 N*m{ 100 kgf*cm , 7 ft.*lbf }

1. Install the shift solenoid valve S1 with the bolt.

   Torque:
     6.4 N*m{ 65 kgf*cm , 56 in.*lbf }

1. Install the shift solenoid valve SR with the 2 bolts.

   Torque:
     6.4 N*m{ 65 kgf*cm , 56 in.*lbf }

1. Install the shift solenoid valve SLU and SL2 with the 2 pins, lock plate and bolt.

   Torque:
     6.4 N*m{ 65 kgf*cm , 56 in.*lbf }

1. Install the shift solenoid valve SLT and SL1 with the 2 pins, lock plate and bolt.

   Torque:
     6.4 N*m{ 65 kgf*cm , 56 in.*lbf }