GSIC - Global Service Information Center

# DECELERATION SENSOR (for 4WD) > REMOVAL

## for Preparation Click here

1. DISCONNECT CABLE FROM NEGATIVE BATTERY TERMINAL

CAUTION:

  Wait at least 90 seconds after disconnecting the cable from the negative (-) battery terminal to prevent airbag and seat belt pretensioner activation.

2. REMOVE FRONT SEAT ASSEMBLY

3. REMOVE DECELERATION SENSOR

1. Remove the bolt and sensor cover.

1. Disconnect the deceleration sensor connector.

1. Remove the 2 nuts and deceleration sensor.