GSIC - Global Service Information Center

# CRANKSHAFT POSITION SENSOR > INSTALLATION

## for Preparation Click here

1. INSTALL CRANKSHAFT POSITION SENSOR

1. Apply a light coat of engine oil to the O-ring of the sensor.

1. Install the sensor with the bolt.

   Torque:
     9.0 N*m{ 92 kgf*cm , 80 in.*lbf }

1. Connect the sensor connector.

2. CONNECT CABLE TO NEGATIVE BATTERY TERMINAL

3. PERFORM INITIALIZATION

1. Perform initialization (Click here).

   NOTICE:
     Certain systems need to be initialized after disconnecting and reconnecting the cable from the negative (-) battery terminal.