GSIC - Global Service Information Center

# EVAPORATOR TEMPERATURE SENSOR > ON-VEHICLE INSPECTION

## for Preparation Click here

1. INSPECT EVAPORATOR TEMPERATURE SENSOR

1. Measure the resistance of the sensor.

   Standard resistance:

     Tester Connection | Condition | Specified Condition
     1 - 2 | 0°C (32°F) | 4.40 to 5.35 kΩ
     1 - 2 | 15°C (59°F) | 2.14 to 2.58 kΩ

   NOTICE:
   1. Even slightly touching the sensor may change the resistance value. Be sure to hold the connector of the sensor.
   2. When measuring, the sensor temperature must be the same as the ambient temperature.

   HINT:
     If the resistance value is not as specified, replace the evaporator temperature sensor.