GSIC - Global Service Information Center

# 1TR-FE FUEL > SERVICE DATA

Fuel pressure : at idle | 281 to 287 kPa (2.87 to 2.93 kgf/cm2, 40.8 to 41.7 psi)
Fuel pressure : Remains as specified for 5 minute after engine stopped | 147 kPa (1.5 kgf/cm2, 21 psi) or more
Fuel injector | Resistance: 11. 6 to 12.4 Ω at 20° (68°F)
Injection volume | 71 to 86 cm3 (4.3 to 5.2 cu, in.) in 5 seconds
Difference between each injector | 15 cm3 (0.9 cu, in.) or less
Fuel pump | Resistance: 0.2 to 3.0 Ω at 20° (68°F)