GSIC - Global Service Information Center

# DIESEL THROTTLE BODY > REMOVAL

## for Preparation Click here

1. DISCONNECT CABLE FROM NEGATIVE BATTERY TERMINAL

CAUTION:

  Wait at least 90 seconds after disconnecting the cable from the negative (-) battery terminal to prevent airbag and seat belt pretensioner activation.

2. REMOVE NO. 1 ENGINE COVER SUB-ASSEMBLY

1. Remove the 3 bolts, 2 nuts and engine cover.

3. REMOVE CHARGE AIR COOLER ASSEMBLY WITH INTAKE AIR CONNECTOR

1. Disconnect the IAT sensor connector and manifold absolute diesel pressure sensor connector.

1. Disconnect the vacuum hose from the manifold absolute pressure sensor.

1. Loosen the 2 clips.

1. Remove the 4 bolts and CAC.

4. REMOVE DIESEL THROTTLE BODY ASSEMBLY

1. Disconnect the 2 connectors.

1. Remove the 2 bolts, 2 nuts, throttle body and gasket.