GSIC - Global Service Information Center

# REAR SEAT INNER BELT ASSEMBLY > INSTALLATION

## for Preparation Click here

1. INSTALL REAR NO. 1 SEAT BELT ASSEMBLY INNER LH (for Double Cab)

1. Install the seat belt with the bolt as shown in the illustration.

   Torque:
     42 N*m{ 428 kgf*cm , 31 ft.*lbf }

   NOTICE:
     Do not overlap the anchor part of the seat belt and protruding parts of the vehicle body.

2. INSTALL REAR NO. 1 SEAT BELT ASSEMBLY INNER RH (for Double Cab)

1. Install the inner seat belt with the bolt as shown in the illustration.

   Torque:
     42 N*m{ 428 kgf*cm , 31 ft.*lbf }

   NOTICE:
     Do not overlap the anchor part of the seat belt and protruding parts of the vehicle body.

3. INSTALL REAR NO. 1 SEAT BELT ASSEMBLY INNER (for Extra Cab)

1. Install the inner seat belt with the bolt as shown in the illustration.

   Torque:
     42 N*m{ 428 kgf*cm , 31 ft.*lbf }

   NOTICE:
     Do not overlap the anchor part of the seat belt and protruding parts of the vehicle body.

4. INSTALL REAR SEAT ASSEMBLY (for Double Cab)

1. Place the seat in the cabin.

   NOTICE:
     Be careful not to damage the vehicle body.

1. Attach the seatback's 2 hooks to the vehicle body.

1. Install the seat with the 4 bolts.

   Torque:
     19.5 N*m{ 199 kgf*cm , 14 ft.*lbf }

   HINT:
     Tighten the bolts in the order indicated in the illustration.

1. Pass the inner belts between the seat cushion and seatback.

1. Fold down the seat cushion.

1. Hook the fold seat stopper band around the knob.