GSIC - Global Service Information Center

# INTAKE AIR TEMPERATURE SENSOR > INSPECTION

## for Preparation Click here

1. INSPECT INTAKE AIR TEMPERATURE SENSOR

1. Measure the resistance between the terminals.

   Standard resistance:
     2.21 to 2.65 Ω at 20°C (68°F)
   If the result is not as specified, replace the sensor.

   NOTICE:
     When checking the ECT sensor in the water, keep the terminals dry. After the check, wipe the sensor dry.