GSIC - Global Service Information Center

### POWER WINDOW CONTROL SYSTEM > Remote Up / Down Function does not Operate

## for Preparation Click here

## DESCRIPTION

Single cab and extra cab:
With the ignition switch ON, the power window regulator master switch transmits remote switch signals to the regulator switch of the passenger door power window. Then, the regulator switch drives its respective power window regulator motor.
Double cab:
With the ignition switch ON, the power window regulator master switch transmits remote switch signals to the regulator switches of the passenger door power window and rear door power windows. Then, each regulator switch drives its respective power window regulator motor.

## WIRING DIAGRAM

## INSPECTION PROCEDURE

1.CHECK POWER WINDOW REGULATOR MASTER SWITCH ASSEMBLY

1. Turn the window lock switch OFF and operate the switches on the master switch. Check that the remote UP / DOWN function operates normally.

   OK:
     Remote UP / DOWN function operates normally.

| NG |

Go to step 2

OK |

END

2.CHECK MANUAL UP / DOWN FUNCTION

1. Single cab and extra cab:
   Check that the passenger door power window manual UP / DOWN function operates normally.
   Double cab:
   Check that the passenger door power window and rear door power window manual UP / DOWN function operates normally.

   OK:
     Manual UP / DOWN function operates normally.

| NG |

OTHER PROBLEM

OK |

REPLACE POWER WINDOW REGULATOR MASTER SWITCH ASSEMBLY