GSIC - Global Service Information Center

# BRAKE PEDAL > REMOVAL

## for Preparation Click here

1. REMOVE COMBINATION METER ASSEMBLY

1. Remove the combination meter (Click here).

2. DISCONNECT BRAKE MASTER CYLINDER PUSH ROD CLEVIS

1. Disconnect the stop light switch connector.

1. Remove the return spring.

1. Remove the clip and clevis pin.

1. Disconnect the push rod clevis from the brake pedal.

3. REMOVE BRAKE PEDAL SUPPORT SUB-ASSEMBLY

1. Remove the bolt from the support.

1. Remove the 4 nuts and support.