GSIC - Global Service Information Center

# CLUTCH PEDAL (for LHD) > REMOVAL

## for Preparation Click here

1. REMOVE INSTRUMENT CLUSTER FINISH PANEL

1. Remove the clip.

1. Detach the 2 claws and remove the panel.

2. REMOVE COMBINATION METER ASSEMBLY

NOTICE:

  There are 2 types of combination meters. One type has a 40 pin connector and 16 pin connector. The other type only has a 40 pin connector.

1. Remove the 3 screws <B>.

1. Disconnect all connectors and remove the combination meter.

3. REMOVE CLUTCH PEDAL RETURN SPRING

1. w/o Turn over:
   Remove the spring.

1. Remove the clip and pin.

4. REMOVE CLUTCH PEDAL ASSEMBLY

1. Remove the bolt, 2 nuts and clutch pedal.